Brand: O/M 
Luminaire name: BS
Model: BS Wall-mounted
Code: 15902
Finishes: .20 Clear

Design: Eduardo Souto de Moura
Emergency luminaire with body made of polycarbonate.
Pictogram, with acrylic structure and adhesive film, supplied separately.
The same luminaire allows maintained or non-maintained mode.
Luminaire with self-testing mode.
Prepared for remote control (rest mode).
3-hour autonomy.
Compliant with the following standards:
EN60598-2-22/ EN60598-1 / UNE 20392 

2,4W / 65lm / 5000K / Product /  / 400x120x85mm

Power supply included.
IP67 | IK08 | 230Vac | 50/60Hz

LOR 19%, UGR -, insulation class II