Brand: O/M 
Luminaire name: LS
Model: LS Wall end mounted
Code: 15905
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .10 Anodised aluminium

Desing: Eduardo Souto de Moura
Emergency wall end mounted luminaire with body made of aluminium profile with matt finish or electrostatic 100% polyester paint with textured-finish.
Pictogram, with acrylic structure and adhesive film, supplied separately.
The same luminaire allows maintained or non-maintained mode.
Luminaire with self-testing mode.
Prepared for remote control (rest mode).
3-hour autonomy.
Compliant with the following standards:
EN60598-2-22 / EN60598-1 / UNE 20392

2,4W / 65lm / 5000K / Product /  / 325x235x60mm

Power supply included.
IP22 | 230Vac | 50/60Hz

LOR 19%, UGR -, insulation class II