Brand: O/M 
Luminaire name: One Plus
Model: One Plus
Code: 60239
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .21 Black+White

Design: O/M + Bartenbach GmbH
Ceiling-recessed luminaire with die-cast aluminium body and heat sink.
Orientable by 30° on the horizontal axis and 355° on the vertical axis.
Reflector built based on micro surfaces with complex geometry coated with aluminium alloy, creating a high-gloss, entirely mirrored surface. Accurate reflector for a defined and controlled beam of light, achieving the maximum efficiency.
Reduced height <67mm.
Recessing accessory for trimless version supplied separately.

4,5W / 560lm /  4000K / On/Off / Flood 56° / ø95mm

LED CRI>80 / >50.000h, L80/B10
2-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 90%, UGR <16, insulation class II