Brand: O/M 
Luminaire name: Beam
Model: Beam IP54
Code: 60392
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing accessory for flush version supplied separately.

2,2W / 170lm /  2700K / On/Off / Spot 14° / ø75mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam / power supply included
IP54 | 230Vac | 50/60Hz

LOR 85%, UGR <10, insulation class II