Brand: O/M 
Luminaire name: Beam
Model: Beam IP54
Code: 60430
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing accessory for flush version supplied separately.

4,5W / 450lm /  4000K / DALI / Flood 37° / ø75mm

LED CRI>80 / >50.000h, L80/B10
2-step MacAdam / power supply included
IP54 | 230Vac | 50/60Hz

LOR 73%, UGR <19, insulation class II