Brand: O/M 
Luminaire name: Dot
Model: Dot
Code: 60475
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .12 Brushed stainless steel, .34 Rust

Design: O/M
Ceiling-recessed luminaire, with aluminium body with 25micron maximum corrosion resistance anodization. Trim aluminium with matt finish or with textured electrostatic 100% polyester paint.
Tempered clear glass.
Supplied with cable (2x0,50mm²).
Driver to be ordered separately.

Values for 700mA. For 350mA estimate half of the indicated values.

2,2W / 180lm /  3000K / On/Off / Flood 41° / Ø36mm

LED CRI>90 / >50.000h, L80/B10 / 3-step MacAdam
IP67 | 350mA / 700mA

LOR 84%, UGR <22, insulation class III