Brand: O/M 
Luminaire name: U60
Model: U60 Recessed
Code: 61482
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .10 Anodised aluminium

Design: Eduardo Souto de Moura
Recessed luminaire with housing made of aluminium profile with 25micron maximum corrosion resistance anodization with matt finish or with textured electrostatic 100% polyester paint. 
Frosted polycarbonate diffuser with user friendly clipping system and double fitting system: flushed or recessed.
Aluminium anodised end caps with matt finish or electrostatic 100% polyester paint with textured-finish.
Fitting accessories ordered separately.

20W / 1725lm / 3000K / On/Off / Diffuse / 1433mm

LED CRI>80 / >50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP42 | 230Vac | 50/60Hz

LOR 48%, UGR <25, insulation class I