Brand: O/M 
Luminaire name: U60
Model: U60 Recessed
Code: 61772
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .10 Anodised aluminium

Design: Eduardo Souto de Moura
Recessed luminaire with housing made of aluminium profile with 25micron maximum corrosion resistance anodization with matt finish or with textured electrostatic 100% polyester paint. 
Prismatic polycarbonate diffuser with low luminance and glare control (UGR<19 for low output or UGR<22 for High Output).
Aluminium anodised end caps with matt finish or electrostatic 100% polyester paint with textured-finish.
Fitting accessories ordered separately.

28W / 3040lm / 3000K / On/Off / Prismatic / 2275mm

LED CRI>80 / >50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP42 | 230Vac | 50/60Hz

LOR 62%, UGR <19, insulation class I