Brand: O/M 
Luminaire name: H45
Model: H45 Pendant
Code: 62211
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .10 Anodised aluminium

Design: O/M
Pendant direct and indirect light luminaire with housing made of anodised aluminium profile with textured paint finish. Frosted diffuser for direct light and clear diffuser for indirect light with user friendly clipping system. 5mm aluminium end caps. 
Separate Circuits. 
Suspension accessories available separately. Supply base made of aluminium, clear power cable (3x0,75mm²) and steel suspension cables (1,5mm) with millimetric height adjustment system.

34+20W / 3300+1480lm / 4000K / DALI / Diffuse / batwing / 1429mm

LED CRI>80 / >50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 54%, UGR <25, insulation class I