Brand: O/M 
Luminaire name: Go
Model: Go Asymmetric
Code: 64751
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing system with spring clips.

6,7W / 3,4W / 580lm / 290lm / 3000K / On/Off / Asymmetric / ø75mm

LED CRI>90 / >50.000h, L80/B10
3-step MacAdam / Power supply not included
IP44 | 200mA / 100mA

LOR 55%, UGR -, insulation class III