Brand: O/M 
Luminaire name: Go
Model: Go IP65
Code: 64828
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing system with spring clips.

3,7W / 310lm / 3500K / On/Off / Flood 60° / ø50mm

LED CRI>90 / >50.000h, L80/B10
3-step MacAdam / Power supply not included
IP65 | 100mA 

LOR 76%, UGR <22, insulation class III