Brand: O/M 
Luminaire name: Go
Model: Go IP65
Code: 64837
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing system with spring clips.
Recessing accessory for flush version supplied separately.

6,7W / 3,4W / 800lm / 400lm / 3000K / On/Off / Medium 34° / ø75mm

LED CRI>90 / >50.000h, L80/B10
3-step MacAdam / Power supply not included
IP65 | 200mA / 100mA

LOR 76%, UGR <16, insulation class III