Brand: O/M 
Luminaire name: Go
Model: Go IP65
Code: 64846
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing system with spring clips.
Recessing accessory for flush version supplied separately.

6,7W / 3,4W / 810lm / 405lm / 4000K / On/Off / Flood 48° / ø75mm

LED CRI>90 / >50.000h, L80/B10
3-step MacAdam / Power supply not included
IP65 | 200mA / 100mA

LOR 76%, UGR <19, insulation class III