Brand: O/M 
Luminaire name: Go
Model: Go IP65
Code: 64848
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing system with spring clips.

10W / 5W / 1130lm / 565lm / 2700K / On/Off / Spot 20° / ø100mm

LED CRI>90 / >50.000h, L80/B10
3-step MacAdam / Power supply not included
IP65 | 300mA / 150mA

LOR 75%, UGR <10, insulation class III