Brand: O/M 
Luminaire name: Nub
Model: Nub
Code: 60002
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Ceiling-recessed luminaire with aluminium die-cast body with electrostatic 100% polyester paint finish. Focal lens with complex surfaces to provide a focal point through an 8mm aperture for low glare illumination. 
Driver to be ordered separately.

5,6W / 280lm / 3000K / On/Off / Medium 33° / ø28mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam
IP65

LOR 61%, UGR <10, insulation class III