Brand: O/M 
Luminaire name: One
Model: One
Code: 60138
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Ceiling-recessed luminaire with aluminium die-cast body and heat sink with electrostatic 100% polyester paint finish. 
Spot-lens with individual complex surface rips to provide a focal light and an extremely narrow beam.
Fitting accessories for different applications are available.

4,5W / 280lm / 2700K / DALI / Spot 15° / ø85mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 58%, UGR <10, insulation class II