Brand: O/M 
Luminaire name: 0v3r2
Model: Over Track
Code: 60274
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Track-mounted spotlight with die-cast aluminium body with electrostatic 100% polyester paint finish.
Spot-lens with individual complex surface rips to provide a focal light and an extremely narrow beam.
Orientable by 90° horizontal rotation and 330° vertical rotation.
Power supply incorporated.

4,5W / 430lm /  2700K / DALI / Flood 59° / ø86mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 90%, UGR 230Vac, insulation class I