Brand: O/M 
Luminaire name: Beam
Model: Beam
Code: 60375
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Recessing accessory for flush version supplied separately.

19W / 1640lm /  3000K / DALI / Medium 28° / ø100mm

LED CRI>80 / >50.000h, L80/B10
3-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 75%, UGR <22, insulation class II