Brand: O/M 
Luminaire name: Uw
Model: Uw Surface/Pendant
Code: 60601
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .10 Anodised aluminium

Design: OM + Bartenbach GmbH
Surface or pendant luminaire with housing made of aluminium with 25 micron maximum corrosion resistance anodization in matte finish or electrostatic 100% polyester paint with textured finish.
Aluminium anodised end caps with matt finish or electrostatic 100% polyester paint with textured-finish.
Linear extruded lenses (Lightstream) combined with a secondary reflector, integrated into an extruded aluminium profile.
Fitting accessories ordered separately. 2200-5000K Tunable White.

16W* / 790lm* / 2200K-5000K / DALI / Wallwasher / 1211mm

LED CRI>80 / >50.000h, L80/B10 / 2-step MacAdam
Power supply included.
DALI DT8
IP20 | 230Vac | 50/60Hz

LOR 46%, UGR -, insulation class I