Brand: O/M 
Luminaire name: U60
Model: U60 IP54 Recessed trimless
Code: 61697
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .10 Anodised aluminium

Design: Eduardo Souto de Moura
Recessed trimless luminaire with housing made of anodised aluminium profile with matt or textured-paint finish.
Frosted polycarbonate diffuser with user friendly clipping system and double fitting system: flushed or recessed.
Aluminium End caps.
Fitting accessories ordered separately.

27W / 2500lm / 4000K / DALI / Diffuse / 1143mm

LED CRI>80 / >50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP54 | 230Vac | 50/60Hz

LOR 48%, UGR <25, insulation class I