Brand: O/M 
Luminaire name: MGB
Model: MGB Pendant indirect
Code: 62333
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .03 Grey / RAL 9006

Design: Eduardo Souto de Moura
Pendant luminaire with housing made of aluminium profile with 25micron maximum corrosion resistance anodization with textured electrostatic 100% polyester paint.  
Frosted acrylic diffuser with user friendly clipping system.
Steel end caps with textured electrostatic 100% polyester paint.
Frosted acrylic diffuser for direct light and indirect light.
Fitting accessories ordered Separately.

126W / 4800lm / 2700K / On/Off / Diffuse indirect / 2970mm

LED CRI>90 />50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 40%, UGR <25, insulation class I