Brand: O/M 
Luminaire name: MGB
Model: MGB Pendant indirect with track
Code: 62358
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .03 Grey / RAL 9006

Design: Eduardo Souto de Moura
Pendant luminaire with housing made of aluminium profile with 25micron maximum corrosion resistance anodization with textured electrostatic 100% polyester paint.
Frosted acrylic diffuser with user friendly clipping system.
Steel end caps with textured electrostatic 100% polyester paint.
Frosted acrylic diffuser for indirect light.
Three-phase track (On/Off or DALI) for installing spotlights.
Fitting accessories ordered separately.

45W / 1700lm / 2700K / DALI / Diffuse indirect / 1560mm

LED CRI>90 />50.000h, L80/B10 / 3-step MacAdam
Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 40%, UGR <25, insulation class I