Brand: O/M 
Luminaire name: Dot
Model: Dot Ground / Concrete
Code: 62730
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .12 Brushed stainless steel, .34 Rust

Design: O/M
Ground-recessed luminaire made of anodised aluminium body with 25-micron maximum corrosion resistance anodization and frame in aluminium matt finish.
Tempered clear glass diffuser.
Recessed housing and driver supplied separately.

Values for 700mA. For 350mA estimate half of the indicated values.

2,2W / 160lm /  3000K / On/Off / Wide flood 75° / Ø36mm

LED CRI>90 / >50.000h, L80/B10 / 3-step MacAdam
IP67 | 350mA / 700mA

LOR 74%, UGR <28, insulation class III