Brand: O/M 
Luminaire name: Beam
Model: Beam Adjustable
Code: 63188
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Adjustable version (orientable by 30° on the horizontal axis and 355° on the vertical axis).
Recessing accessory for flush version supplied separately.

4,5W / 360lm /  2700K / DALI / Flood 37° / ø75mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 75%, UGR <19, insulation class II