Brand: O/M 
Luminaire name: Beam
Model: Beam Adjustable
Code: 63213
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Adjustable version (orientable by 30° on the horizontal axis and 355° on the vertical axis).
Recessing accessory for flush version supplied separately.

19W / 1630lm /  2700K / On/Off / Flood 46° / ø100mm

LED CRI>90 / >50.000h, L80/B10
3-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 79%, UGR <22, insulation class II