Brand: O/M 
Luminaire name: Beam
Model: Beam Adjustable
Code: 63219
Finishes: .04 Matt White, .05 Matt Black

Design: O/M
Ceiling-recessed luminaire made of aluminium die-cast.
Adjustable version (orientable by 30° on the horizontal axis and 355° on the vertical axis).
Recessing accessory for flush version supplied separately.

19W / 1640lm /  3000K / On/Off / Medium 28° / ø100mm

LED CRI>80 / >50.000h, L80/B10
3-step MacAdam / Power supply included.
IP20 | 230Vac | 50/60Hz

LOR 75%, UGR <22, insulation class II