Brand: O/M 
Luminaire name: Tua
Model: Tua Optic
Code: 64605
Finishes: .01 White / RAL 9010, .02 Black / RAL 9005, .33 Graphite Black, .34 Rust

Design: O/M + Eduardo Souto de Moura
Outdoor luminaire in aluminium body with anti-corrosion treatment and textured electrostatic 100% polyester paint finish.
Clear glass diffuser.
Asymmetrical aluminium reflector with 97% reflection, low luminance level and low UGR level.
Fitting accessory available separately.

*Polycarbonate clear diffuser (IK10) available under request.

7,3W / 480lm / 4000K / DALI / Elliptical longitudinal / 252x200x65mm

LED CRI>80 / >50.000h, L80/B10
2-step MacAdam / power supply included.
IP66 | 230Vac | 50/60Hz

LOR 53%, UGR -, insulation class I