Brand: O/M 
Luminaire name: Nub
Model: Nub Flush 
Code: 64945
Finishes: .02 Black / RAL 9005

Design: O/M + Bartenbach GmbH
Ceiling-recessed luminaire with aluminium die-cast body with electrostatic 100% polyester paint finish.
Focal-lens with complex surfaces to provide a focal point through an 8mm aperture for low glare illumination.
Supplied with fermacell® plasterboard fiber recessing accessory or plasterboard.
Driver to be ordered separately.

2,1W / 100lm / 3000K / On/Off / Spot 16° / 8mm

LED CRI>90 / >50.000h, L80/B10
2-step MacAdam
IP65

LOR 50%, UGR <19, insulation class III